# Uncertainty Analysis in Dynamic Site and Slope Response

## Documentation for package ‘newmark’ version 1.1.0

- DESCRIPTION file.
- User guides, package vignettes and other documentation.
- Package NEWS.

## Help Pages

approx.spline | Highcharts-style cubic spline interpolation
buildGMDP | Build Ground-Motion Design Parameters (GMDP)
buildQSpline | Build a monotone quantile spline Q(u) for ln(Sa)
checkUHS | Check monotonicity and duplicates in UHSTable
CylinderRoots | Cylinder Roots Data
designUHS | MCER / Design elastic spectrum for a Vs30/Vref slice (ASCE 7-22)
Dn_AM88 | Ambraseys & Menu (1988) rigid sliding-block model
Dn_BM17 | Bray & Macedo (2017) - subduction/interface events
Dn_BM19 | Bray & Macedo (2019, corrected 2023) - shallow-crustal events
Dn_BT07 | Bray & Travasarou (2007) flexible sliding-block model
Dn_JB07 | Jibson (2007) empirical model
Dn_SR08 | Saygili & Rathje (2008) model
fitDnCurve | Newmark displacement curve Dn(ky) for one scenario
fitDnModel | Newmark displacement for a single submodel and scenario
fitModel.Ts | Site's Fundamental Period
fitSaF | Site-amplified AUXtral acceleration (Seyhan & Stewart 2014)
F_ST17 | Non-linear site amplification factor *FST17*
geSiteTable | Single-realisation synthetic soil profile and site properties
getCylinderRoots | Characteristic root of an inhomogeneous truncated shear beam
getDnKy | Build a log-spaced ky grid for one scenario
getKyLimits | Get calibrated ky range for each displacement model
getSiteProperties | Monte Carlo site properties from synthetic soil profiles
interpolateSaTable | Interpolate Sa(p) at arbitrary period using log-log interpolation
invertDnDraws | Invert Dn draws to kmax(Da)
rhoBJ | Baker and Jayaram (2008) inter-period correlation model
SaF_ST17 | Site-amplified spectral acceleration using Seyhan & Stewart (2014)
sampleSaCorr | Draw a correlated sample of spectral accelerations
ShearModelParameters | ShearModelParameters
SIDtoVs30 | Convert Site Class to Vs30 in m/s
SiteClass | Site Class Data
SiteTable | SiteTable Data
Vs30toSID | Convert Vs30 (m/s) to Site Class Identifier