# Environmental Noise Pollution Data Analysis

## Documentation for package ‘OpeNoise’ version 0.2-18

- DESCRIPTION file
- Package NEWS
- Package README

## Help Pages

AcousticQuantilePlot | Plot acoustic quantile
AcousticWeightingTable | Weighting acoustic table
AcuDNPercentile | Calculate reverse Percentile for period
AcuPercentile | Calculate reverse Percentile
avr.day.night | Calculate daily and nightly energetic mean period
dataset_impulsive1 | Noise dataset of impulsive event (100 ms acquisition time)
dataset_impulsive2 | Noise dataset of impulsive event (100 ms acquisition time)
dbsum | Calculate energetic sum or difference of values
deco.time | Time decomposition
dfBW | Table's 1/3 octave bandwidth
dfImpulsiveTrasform | Trasform impulsive dataframe (100 ms samples) in dataframe (1s samples)
energetic.mean | Logarithmic mean
energetic.min | Function that calculate min value
energetic_w.mean | Weigth logaritmic mean
exampleHourlyData | Noise hourly data of misure in environmental open space
ExtractIndexMark | Extract index and name of markers
HolidaysDate | Calculate Holidays date (Gregorian calendar)
HourlyEmean | Calculate hourly energetic mean
IntrusiveIndex | Calculate Intrusive Index (UNI/TS 11844 march 2022)
iso | Parameters table of equal loudness curve A (ISO 226:1987 “Acoustics - Normal equal-loudness-level contours”)
LdenCalculator | Calculate daily or total Lden (Day-evening-night level)
markers | Dataset with markers
Maskapply | Add index and name of markers in misure dataframe
P1FA | Noise data of misure in house open window condition
P1FC | Noise data of misure in house close window condition
PlotNoiseTHcompare | Plot time history and compare frequency components
PlotNoiseTimeHistory | Plot time history of noise misure with marker and running Leq
PlotSpectrogram | Plot spectrogram
PTFA | Noise data of misure in house open window condition
PTFC | Noise data of misure in house close window condition
RoundTo | Round to Multiple
runningLeq | Calculate running Leq
search.tone | Function research pure tone
searchImpulse | Search impulsive event
SELcalc | Calculate SEL (Single Event Level)